MUSIC AND PAGING MIXER/PROCESSOR

━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━━

(1) 기능

본 기기는 음악 및 페이징 믹서/프로세서로서 4개의 마이크/라인입력, 4개의 모노 라인입력 및 4개의 출력을 지원하며 USB 포트를 지원하고 외부 제어 트리거 용 입력 2개를 지원하며 사용자 제어 응용 프로그램으로 엑세스하기 위해 이더넷 포트가 지원되어야 한다. 기기를 컨트롤하기 위한 앱이 지원되며 존 레벨 제어 및 소스 선택, 프리셋 불러오기, 스케줄링 및 믹서 제어가 지원되어야 한다.

(2) 기기특성

[Inputs]

- Total	: 8

- Mic/line	: 4(euroblock)

- RCA	: 4(mono-summed RCA pairs)

- Stereo USB	: Stereo USB/MP3 playback

[Outputs]

- Total	: 6

- Line	: 4(euroblock, balanced)

- Music-on-hold	: 1(euroblock, transformer balanced)

- Cue(phones)	: 1(3.5mm, stereo)

[Audio]

- Sampling frequency	: 48kHz

- Processing	: 32-bit floating point

- THD	: <0.005%, +4dBu and –2dBr;
20Hz~20kHz, unity gain,
any input to any output

- Frequency response	: 20Hz~20kHz +/-0.5dB,
mic/line or line input to any line
output

- Dynamic range	: > 106dB unweighted

- Crosstalk	> 90dB typical, > 80dB max

- Gain(mic inputs)	: 51dB

- Maximum input level	: +24dBu(mic/line inputs),
+10dBV(line inputs)

- Maximum output level	: +21dBu(line-level outputs),
+10dBV(music on hold)

- Phantom power	: All microphone inputs(+12volts)

- Latency	: 2.3msec

[Input processing]

- EQ	: 1/3 octave GEQ

Anti-frrdback filters	: 12-band variable notch filters

- Dynamics	: Gate, choice of AGC

(Auto Gain Control) or compressor

[Output processing]

- EQ	: 1/3 octave GEQ

- Anti-feedback filters	: 12-band variable notch filters

- Dynamics	: Comp/limiter, ducker, loudness

- Delay	: 100msec

- Loudspeaker tunings

Factory	: Intrinsic correction™
voicing for QSC loudspeakers
User	: 6-band parametric EQ,
HPF&LPF(Linkwitz-Riley or
Butterworth; 12, 18 or

24dB/octave)

[Other Connections]

- Ethernet	: 1 x RJ45 for connection to Wi-Fi
router(user supplied)

- MP-MFC ports	: 2 x RJ45

- USB	: 2 USB-A(firmware&configuration
uploads, USB Wi-Fi)

- GPI	: 2inputs(euroblock)

- Power requirements	: 100~240 VAC, 50~60Hz, universal
supply, IEC inlet

- Indicators	: Blue power LED, blue statys
LED

- Dimensions

Net	: 1.75in x 19in x 14in
(4.5cm x 48.3cm x 35.6cm)

- Weight

Shipping	: 11.0lb(5.0kg)

Net	: 7.0lb(3.2kg)

** MP-M40 또는 동등 이상품 이어야 한다.